Static Call Graph - [.\Obj\USERAPP.axf]

# Static Call Graph for image .\Obj\USERAPP.axf

#<CALLGRAPH># ARM Linker, 5.03 [Build 24]: Last Updated: Tue Jan 26 22:02:57 2016

### Maximum Stack Usage = 112 bytes + Unknown(Cycles, Untraceable Function Pointers)

### Call chain for Maximum Stack Depth:

main ⇒ LCD_Print ⇒ LCD_P16x16Str ⇒ LCD_Set_Pos ⇒ LCD_WrCmd

### Mutually Recursive functions

- BusFaultException ⇒ BusFaultException
- HardFaultException ⇒ HardFaultException
- MemManageException ⇒ MemManageException
- UsageFaultException ⇒ UsageFaultException

  ### Function Pointers

  - ADC1_2_IRQHandler from stm32f10x_it.o(i.ADC1_2_IRQHandler) referenced from stm32f10x_vector.o(RESET)
  - ADC3_IRQHandler from stm32f10x_it.o(i.ADC3_IRQHandler) referenced from stm32f10x_vector.o(RESET)
  - BusFaultException from stm32f10x_it.o(i.BusFaultException) referenced from stm32f10x_vector.o(RESET)
  - CAN_RX1_IRQHandler from stm32f10x_it.o(i.CAN_RX1_IRQHandler) referenced from stm32f10x_vector.o(RESET)
  - CAN_SCE_IRQHandler from stm32f10x_it.o(i.CAN_SCE_IRQHandler) referenced from stm32f10x_vector.o(RESET)
  - DMA1_Channel1_IRQHandler from stm32f10x_it.o(i.DMA1_Channel1_IRQHandler) referenced from stm32f10x_vector.o(RESET)
  - DMA1_Channel2_IRQHandler from stm32f10x_it.o(i.DMA1_Channel2_IRQHandler) referenced from stm32f10x_vector.o(RESET)
  - DMA1_Channel3_IRQHandler from stm32f10x_it.o(i.DMA1_Channel3_IRQHandler) referenced from stm32f10x_vector.o(RESET)
  - DMA1_Channel4_IRQHandler from stm32f10x_it.o(i.DMA1_Channel4_IRQHandler) referenced from stm32f10x_vector.o(RESET)
  - DMA1_Channel5_IRQHandler from stm32f10x_it.o(i.DMA1_Channel5_IRQHandler) referenced from stm32f10x_vector.o(RESET)
  - DMA1_Channel6_IRQHandler from stm32f10x_it.o(i.DMA1_Channel6_IRQHandler) referenced from stm32f10x_vector.o(RESET)
  - DMA1_Channel7_IRQHandler from stm32f10x_it.o(i.DMA1_Channel7_IRQHandler) referenced from stm32f10x_vector.o(RESET)
  - DMA2_Channel1_IRQHandler from stm32f10x_it.o(i.DMA2_Channel1_IRQHandler) referenced from stm32f10x_vector.o(RESET)
  - DMA2_Channel2_IRQHandler from stm32f10x_it.o(i.DMA2_Channel2_IRQHandler) referenced from stm32f10x_vector.o(RESET)
  - DMA2_Channel3_IRQHandler from stm32f10x_it.o(i.DMA2_Channel3_IRQHandler) referenced from stm32f10x_vector.o(RESET)
  - DMA2_Channel4_5_IRQHandler from stm32f10x_it.o(i.DMA2_Channel4_5_IRQHandler) referenced from stm32f10x_vector.o(RESET)
  - DebugMonitor from stm32f10x_it.o(i.DebugMonitor) referenced from stm32f10x_vector.o(RESET)
  - EXTI0_IRQHandler from stm32f10x_it.o(i.EXTI0_IRQHandler) referenced from stm32f10x_vector.o(RESET)
  - EXTI15_10_IRQHandler from stm32f10x_it.o(i.EXTI15_10_IRQHandler) referenced from stm32f10x_vector.o(RESET)
  - EXTI1_IRQHandler from stm32f10x_it.o(i.EXTI1_IRQHandler) referenced from stm32f10x_vector.o(RESET)
  - EXTI2_IRQHandler from stm32f10x_it.o(i.EXTI2_IRQHandler) referenced from stm32f10x_vector.o(RESET)
  - EXTI3_IRQHandler from stm32f10x_it.o(i.EXTI3_IRQHandler) referenced from stm32f10x_vector.o(RESET)
  - EXTI4_IRQHandler from stm32f10x_it.o(i.EXTI4_IRQHandler) referenced from stm32f10x_vector.o(RESET)
  - EXTI9_5_IRQHandler from stm32f10x_it.o(i.EXTI9_5_IRQHandler) referenced from stm32f10x_vector.o(RESET)
  - FLASH_IRQHandler from stm32f10x_it.o(i.FLASH_IRQHandler) referenced from stm32f10x_vector.o(RESET)
  - FSMC_IRQHandler from stm32f10x_it.o(i.FSMC_IRQHandler) referenced from stm32f10x_vector.o(RESET)
  - HardFaultException from stm32f10x_it.o(i.HardFaultException) referenced from stm32f10x_vector.o(RESET)
  - I2C1_ER_IRQHandler from stm32f10x_it.o(i.I2C1_ER_IRQHandler) referenced from stm32f10x_vector.o(RESET)
  - I2C1_EV_IRQHandler from stm32f10x_it.o(i.I2C1_EV_IRQHandler) referenced from stm32f10x_vector.o(RESET)
  - I2C2_ER_IRQHandler from stm32f10x_it.o(i.I2C2_ER_IRQHandler) referenced from stm32f10x_vector.o(RESET)
  - I2C2_EV_IRQHandler from stm32f10x_it.o(i.I2C2_EV_IRQHandler) referenced from stm32f10x_vector.o(RESET)
  - MemManageException from stm32f10x_it.o(i.MemManageException) referenced from stm32f10x_vector.o(RESET)
  - NMIException from stm32f10x_it.o(i.NMIException) referenced from stm32f10x_vector.o(RESET)
  - PVD_IRQHandler from stm32f10x_it.o(i.PVD_IRQHandler) referenced from stm32f10x_vector.o(RESET)
  - PendSVC from stm32f10x_it.o(i.PendSVC) referenced from stm32f10x_vector.o(RESET)
  - RCC_IRQHandler from stm32f10x_it.o(i.RCC_IRQHandler) referenced from stm32f10x_vector.o(RESET)
  - RTCAlarm_IRQHandler from stm32f10x_it.o(i.RTCAlarm_IRQHandler) referenced from stm32f10x_vector.o(RESET)
  - RTC_IRQHandler from stm32f10x_it.o(i.RTC_IRQHandler) referenced from stm32f10x_vector.o(RESET)
  - Reset_Handler from stm32f10x_vector.o(.text) referenced from stm32f10x_vector.o(RESET)
  - SDIO_IRQHandler from stm32f10x_it.o(i.SDIO_IRQHandler) referenced from stm32f10x_vector.o(RESET)
  - SPI1_IRQHandler from stm32f10x_it.o(i.SPI1_IRQHandler) referenced from stm32f10x_vector.o(RESET)
  - SPI2_IRQHandler from stm32f10x_it.o(i.SPI2_IRQHandler) referenced from stm32f10x_vector.o(RESET)
  - SPI3_IRQHandler from stm32f10x_it.o(i.SPI3_IRQHandler) referenced from stm32f10x_vector.o(RESET)
  - SVCHandler from stm32f10x_it.o(i.SVCHandler) referenced from stm32f10x_vector.o(RESET)
  - SysTickHandler from stm32f10x_it.o(i.SysTickHandler) referenced from stm32f10x_vector.o(RESET)
  - TAMPER_IRQHandler from stm32f10x_it.o(i.TAMPER_IRQHandler) referenced from stm32f10x_vector.o(RESET)
  - TIM1_BRK_IRQHandler from stm32f10x_it.o(i.TIM1_BRK_IRQHandler) referenced from stm32f10x_vector.o(RESET)
  - TIM1_CC_IRQHandler from stm32f10x_it.o(i.TIM1_CC_IRQHandler) referenced from stm32f10x_vector.o(RESET)
  - TIM1_TRG_COM_IRQHandler from stm32f10x_it.o(i.TIM1_TRG_COM_IRQHandler) referenced from stm32f10x_vector.o(RESET)
  - TIM1_UP_IRQHandler from stm32f10x_it.o(i.TIM1_UP_IRQHandler) referenced from stm32f10x_vector.o(RESET)
  - TIM2_IRQHandler from stm32f10x_it.o(i.TIM2_IRQHandler) referenced from stm32f10x_vector.o(RESET)
  - TIM3_IRQHandler from stm32f10x_it.o(i.TIM3_IRQHandler) referenced from stm32f10x_vector.o(RESET)
  - TIM4_IRQHandler from stm32f10x_it.o(i.TIM4_IRQHandler) referenced from stm32f10x_vector.o(RESET)
  - TIM5_IRQHandler from stm32f10x_it.o(i.TIM5_IRQHandler) referenced from stm32f10x_vector.o(RESET)
  - TIM6_IRQHandler from stm32f10x_it.o(i.TIM6_IRQHandler) referenced from stm32f10x_vector.o(RESET)
  - TIM7_IRQHandler from stm32f10x_it.o(i.TIM7_IRQHandler) referenced from stm32f10x_vector.o(RESET)
  - TIM8_BRK_IRQHandler from stm32f10x_it.o(i.TIM8_BRK_IRQHandler) referenced from stm32f10x_vector.o(RESET)
  - TIM8_CC_IRQHandler from stm32f10x_it.o(i.TIM8_CC_IRQHandler) referenced from stm32f10x_vector.o(RESET)
  - TIM8_TRG_COM_IRQHandler from stm32f10x_it.o(i.TIM8_TRG_COM_IRQHandler) referenced from stm32f10x_vector.o(RESET)
  - TIM8_UP_IRQHandler from stm32f10x_it.o(i.TIM8_UP_IRQHandler) referenced from stm32f10x_vector.o(RESET)
  - UART4_IRQHandler from stm32f10x_it.o(i.UART4_IRQHandler) referenced from stm32f10x_vector.o(RESET)
  - UART5_IRQHandler from stm32f10x_it.o(i.UART5_IRQHandler) referenced from stm32f10x_vector.o(RESET)
  - USART1_IRQHandler from stm32f10x_it.o(i.USART1_IRQHandler) referenced from stm32f10x_vector.o(RESET)
  - USART2_IRQHandler from stm32f10x_it.o(i.USART2_IRQHandler) referenced from stm32f10x_vector.o(RESET)
  - USART3_IRQHandler from stm32f10x_it.o(i.USART3_IRQHandler) referenced from stm32f10x_vector.o(RESET)
  - USBWakeUp_IRQHandler from stm32f10x_it.o(i.USBWakeUp_IRQHandler) referenced from stm32f10x_vector.o(RESET)
  - USB_HP_CAN_TX_IRQHandler from stm32f10x_it.o(i.USB_HP_CAN_TX_IRQHandler) referenced from stm32f10x_vector.o(RESET)
  - USB_LP_CAN_RX0_IRQHandler from stm32f10x_it.o(i.USB_LP_CAN_RX0_IRQHandler) referenced from stm32f10x_vector.o(RESET)
  - UsageFaultException from stm32f10x_it.o(i.UsageFaultException) referenced from stm32f10x_vector.o(RESET)
  - WWDG_IRQHandler from stm32f10x_it.o(i.WWDG_IRQHandler) referenced from stm32f10x_vector.o(RESET)
  - __main from entry.o(.ARM.Collect$$$$00000000) referenced from stm32f10x_vector.o(.text)
  - main from main.o(i.main) referenced from entry9a.o(.ARM.Collect$$$$0000000B)

  ### Global Symbols

  __main (Thumb, 0 bytes, Stack size unknown bytes, entry.o(.ARM.Collect$$$$00000000))
  [Address Reference Count : 1]

  - stm32f10x_vector.o(.text)

  _main_stk (Thumb, 0 bytes, Stack size unknown bytes, entry2.o(.ARM.Collect$$$$00000001))

  _main_scatterload (Thumb, 0 bytes, Stack size unknown bytes, entry5.o(.ARM.Collect$$$$00000004))
  [Calls]

  - >> __scatterload

  __main_after_scatterload (Thumb, 0 bytes, Stack size unknown bytes, entry5.o(.ARM.Collect$$$$00000004))
  [Called By]

  - >> __scatterload

  _main_clock (Thumb, 0 bytes, Stack size unknown bytes, entry7b.o(.ARM.Collect$$$$00000008))

  _main_cpp_init (Thumb, 0 bytes, Stack size unknown bytes, entry8b.o(.ARM.Collect$$$$0000000A))

  _main_init (Thumb, 0 bytes, Stack size unknown bytes, entry9a.o(.ARM.Collect$$$$0000000B))

  __rt_final_cpp (Thumb, 0 bytes, Stack size unknown bytes, entry10a.o(.ARM.Collect$$$$0000000D))

  __rt_final_exit (Thumb, 0 bytes, Stack size unknown bytes, entry11a.o(.ARM.Collect$$$$0000000F))

  Reset_Handler (Thumb, 4 bytes, Stack size 0 bytes, stm32f10x_vector.o(.text))
  [Address Reference Count : 1]

  - stm32f10x_vector.o(RESET)

  __scatterload (Thumb, 28 bytes, Stack size 0 bytes, init.o(.text))
  [Calls]

  - >> __main_after_scatterload
  [Called By]
  - >> _main_scatterload

  __scatterload_rt2 (Thumb, 0 bytes, Stack size 0 bytes, init.o(.text), UNUSED)

  ADC1_2_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.ADC1_2_IRQHandler))
  [Address Reference Count : 1]

  - stm32f10x_vector.o(RESET)

  ADC3_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.ADC3_IRQHandler))
  [Address Reference Count : 1]

  - stm32f10x_vector.o(RESET)

  BusFaultException (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.BusFaultException))
  [Calls]

  - >> BusFaultException
  [Called By]
  - >> BusFaultException
  [Address Reference Count : 1]
  - stm32f10x_vector.o(RESET)

  CAN_RX1_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.CAN_RX1_IRQHandler))
  [Address Reference Count : 1]

  - stm32f10x_vector.o(RESET)

  CAN_SCE_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.CAN_SCE_IRQHandler))
  [Address Reference Count : 1]

  - stm32f10x_vector.o(RESET)

  DMA1_Channel1_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.DMA1_Channel1_IRQHandler))
  [Address Reference Count : 1]

  - stm32f10x_vector.o(RESET)

  DMA1_Channel2_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.DMA1_Channel2_IRQHandler))
  [Address Reference Count : 1]

  - stm32f10x_vector.o(RESET)

  DMA1_Channel3_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.DMA1_Channel3_IRQHandler))
  [Address Reference Count : 1]

  - stm32f10x_vector.o(RESET)

  DMA1_Channel4_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.DMA1_Channel4_IRQHandler))
  [Address Reference Count : 1]

  - stm32f10x_vector.o(RESET)

  DMA1_Channel5_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.DMA1_Channel5_IRQHandler))
  [Address Reference Count : 1]

  - stm32f10x_vector.o(RESET)

  DMA1_Channel6_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.DMA1_Channel6_IRQHandler))
  [Address Reference Count : 1]

  - stm32f10x_vector.o(RESET)

  DMA1_Channel7_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.DMA1_Channel7_IRQHandler))
  [Address Reference Count : 1]

  - stm32f10x_vector.o(RESET)

  DMA2_Channel1_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.DMA2_Channel1_IRQHandler))
  [Address Reference Count : 1]

  - stm32f10x_vector.o(RESET)

  DMA2_Channel2_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.DMA2_Channel2_IRQHandler))
  [Address Reference Count : 1]

  - stm32f10x_vector.o(RESET)

  DMA2_Channel3_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.DMA2_Channel3_IRQHandler))
  [Address Reference Count : 1]

  - stm32f10x_vector.o(RESET)

  DMA2_Channel4_5_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.DMA2_Channel4_5_IRQHandler))
  [Address Reference Count : 1]

  - stm32f10x_vector.o(RESET)

  DebugMonitor (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.DebugMonitor))
  [Address Reference Count : 1]

  - stm32f10x_vector.o(RESET)

  Draw_BMP (Thumb, 70 bytes, Stack size 24 bytes, oled.o(i.Draw_BMP))
  [Stack]

  - Max Depth = 48
  - Call Chain = Draw_BMP ⇒ LCD_Set_Pos ⇒ LCD_WrCmd
  [Calls]
  - >> LCD_WrDat
  - >> LCD_Set_Pos
  [Called By]
  - >> main

  EXTI0_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.EXTI0_IRQHandler))
  [Address Reference Count : 1]

  - stm32f10x_vector.o(RESET)

  EXTI15_10_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.EXTI15_10_IRQHandler))
  [Address Reference Count : 1]

  - stm32f10x_vector.o(RESET)

  EXTI1_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.EXTI1_IRQHandler))
  [Address Reference Count : 1]

  - stm32f10x_vector.o(RESET)

  EXTI2_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.EXTI2_IRQHandler))
  [Address Reference Count : 1]

  - stm32f10x_vector.o(RESET)

  EXTI3_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.EXTI3_IRQHandler))
  [Address Reference Count : 1]

  - stm32f10x_vector.o(RESET)

  EXTI4_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.EXTI4_IRQHandler))
  [Address Reference Count : 1]

  - stm32f10x_vector.o(RESET)

  EXTI9_5_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.EXTI9_5_IRQHandler))
  [Address Reference Count : 1]

  - stm32f10x_vector.o(RESET)

  EXTI_Configuration (Thumb, 2 bytes, Stack size 0 bytes, gpio.o(i.EXTI_Configuration))
  [Called By]

  - >> main

  FLASH_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.FLASH_IRQHandler))
  [Address Reference Count : 1]

  - stm32f10x_vector.o(RESET)

  FLASH_PrefetchBufferCmd (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_flash.o(i.FLASH_PrefetchBufferCmd))
  [Called By]

  - >> RCC_Configuration

  FLASH_SetLatency (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_flash.o(i.FLASH_SetLatency))
  [Called By]

  - >> RCC_Configuration

  FSMC_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.FSMC_IRQHandler))
  [Address Reference Count : 1]

  - stm32f10x_vector.o(RESET)

  GPIO_Configuration (Thumb, 54 bytes, Stack size 8 bytes, gpio.o(i.GPIO_Configuration))
  [Stack]

  - Max Depth = 28
  - Call Chain = GPIO_Configuration ⇒ GPIO_PinRemapConfig
  [Calls]
  - >> RCC_APB2PeriphClockCmd
  - >> GPIO_PinRemapConfig
  - >> GPIO_Init
  [Called By]
  - >> GPIO_UserInit

  GPIO_Init (Thumb, 152 bytes, Stack size 20 bytes, stm32f10x_gpio.o(i.GPIO_Init))
  [Stack]

  - Max Depth = 20
  - Call Chain = GPIO_Init
  [Called By]
  - >> GPIO_Configuration

  GPIO_PinRemapConfig (Thumb, 66 bytes, Stack size 20 bytes, stm32f10x_gpio.o(i.GPIO_PinRemapConfig))
  [Stack]

  - Max Depth = 20
  - Call Chain = GPIO_PinRemapConfig
  [Called By]
  - >> GPIO_Configuration

  GPIO_ResetBits (Thumb, 4 bytes, Stack size 0 bytes, stm32f10x_gpio.o(i.GPIO_ResetBits))
  [Called By]

  - >> LCD_WrDat
  - >> LCD_WrCmd
  - >> LCD_Init

  GPIO_SetBits (Thumb, 4 bytes, Stack size 0 bytes, stm32f10x_gpio.o(i.GPIO_SetBits))
  [Called By]

  - >> LCD_WrDat
  - >> LCD_WrCmd
  - >> LCD_Init

  GPIO_UserInit (Thumb, 4 bytes, Stack size 0 bytes, gpio.o(i.GPIO_UserInit))
  [Stack]

  - Max Depth = 28
  - Call Chain = GPIO_UserInit ⇒ GPIO_Configuration ⇒ GPIO_PinRemapConfig
  [Calls]
  - >> GPIO_Configuration
  [Called By]
  - >> main

  HardFaultException (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.HardFaultException))
  [Calls]

  - >> HardFaultException
  [Called By]
  - >> HardFaultException
  [Address Reference Count : 1]
  - stm32f10x_vector.o(RESET)

  I2C1_ER_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.I2C1_ER_IRQHandler))
  [Address Reference Count : 1]

  - stm32f10x_vector.o(RESET)

  I2C1_EV_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.I2C1_EV_IRQHandler))
  [Address Reference Count : 1]

  - stm32f10x_vector.o(RESET)

  I2C2_ER_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.I2C2_ER_IRQHandler))
  [Address Reference Count : 1]

  - stm32f10x_vector.o(RESET)

  I2C2_EV_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.I2C2_EV_IRQHandler))
  [Address Reference Count : 1]

  - stm32f10x_vector.o(RESET)

  LCD_DLY_ms (Thumb, 28 bytes, Stack size 0 bytes, oled.o(i.LCD_DLY_ms))
  [Called By]

  - >> LCD_Init

  LCD_Fill (Thumb, 54 bytes, Stack size 16 bytes, oled.o(i.LCD_Fill))
  [Stack]

  - Max Depth = 32
  - Call Chain = LCD_Fill ⇒ LCD_WrDat
  [Calls]
  - >> LCD_WrDat
  - >> LCD_WrCmd
  [Called By]
  - >> LCD_Init

  LCD_Init (Thumb, 220 bytes, Stack size 8 bytes, oled.o(i.LCD_Init))
  [Stack]

  - Max Depth = 40
  - Call Chain = LCD_Init ⇒ LCD_Fill ⇒ LCD_WrDat
  [Calls]
  - >> GPIO_SetBits
  - >> GPIO_ResetBits
  - >> LCD_WrCmd
  - >> LCD_Set_Pos
  - >> LCD_Fill
  - >> LCD_DLY_ms
  [Called By]
  - >> main

  LCD_P16x16Str (Thumb, 232 bytes, Stack size 40 bytes, oled.o(i.LCD_P16x16Str))
  [Stack]

  - Max Depth = 64
  - Call Chain = LCD_P16x16Str ⇒ LCD_Set_Pos ⇒ LCD_WrCmd
  [Calls]
  - >> LCD_WrDat
  - >> LCD_Set_Pos
  [Called By]
  - >> LCD_Print

  LCD_P6x8Str (Thumb, 86 bytes, Stack size 32 bytes, oled.o(i.LCD_P6x8Str))
  [Stack]

  - Max Depth = 56
  - Call Chain = LCD_P6x8Str ⇒ LCD_Set_Pos ⇒ LCD_WrCmd
  [Calls]
  - >> LCD_WrDat
  - >> LCD_Set_Pos
  [Called By]
  - >> LCD_Print

  LCD_P8x16Str (Thumb, 112 bytes, Stack size 32 bytes, oled.o(i.LCD_P8x16Str))
  [Stack]

  - Max Depth = 56
  - Call Chain = LCD_P8x16Str ⇒ LCD_Set_Pos ⇒ LCD_WrCmd
  [Calls]
  - >> LCD_WrDat
  - >> LCD_Set_Pos
  [Called By]
  - >> LCD_Print

  LCD_Print (Thumb, 124 bytes, Stack size 40 bytes, oled.o(i.LCD_Print))
  [Stack]

  - Max Depth = 104
  - Call Chain = LCD_Print ⇒ LCD_P16x16Str ⇒ LCD_Set_Pos ⇒ LCD_WrCmd
  [Calls]
  - >> LCD_P8x16Str
  - >> LCD_P6x8Str
  - >> LCD_P16x16Str
  [Called By]
  - >> main

  LCD_Set_Pos (Thumb, 42 bytes, Stack size 8 bytes, oled.o(i.LCD_Set_Pos))
  [Stack]

  - Max Depth = 24
  - Call Chain = LCD_Set_Pos ⇒ LCD_WrCmd
  [Calls]
  - >> LCD_WrCmd
  [Called By]
  - >> LCD_P8x16Str
  - >> LCD_P6x8Str
  - >> LCD_P16x16Str
  - >> LCD_Init
  - >> Draw_BMP

  LCD_WrCmd (Thumb, 78 bytes, Stack size 16 bytes, oled.o(i.LCD_WrCmd))
  [Stack]

  - Max Depth = 16
  - Call Chain = LCD_WrCmd
  [Calls]
  - >> GPIO_SetBits
  - >> GPIO_ResetBits
  [Called By]
  - >> LCD_Set_Pos
  - >> LCD_Fill
  - >> LCD_Init

  LCD_WrDat (Thumb, 78 bytes, Stack size 16 bytes, oled.o(i.LCD_WrDat))
  [Stack]

  - Max Depth = 16
  - Call Chain = LCD_WrDat
  [Calls]
  - >> GPIO_SetBits
  - >> GPIO_ResetBits
  [Called By]
  - >> LCD_P8x16Str
  - >> LCD_P6x8Str
  - >> LCD_P16x16Str
  - >> LCD_Fill
  - >> Draw_BMP

  MemManageException (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.MemManageException))
  [Calls]

  - >> MemManageException
  [Called By]
  - >> MemManageException
  [Address Reference Count : 1]
  - stm32f10x_vector.o(RESET)

  NMIException (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.NMIException))
  [Address Reference Count : 1]

  - stm32f10x_vector.o(RESET)

  NVIC_Configuration (Thumb, 34 bytes, Stack size 8 bytes, gpio.o(i.NVIC_Configuration))
  [Stack]

  - Max Depth = 20
  - Call Chain = NVIC_Configuration ⇒ NVIC_SystemHandlerPriorityConfig
  [Calls]
  - >> NVIC_SystemHandlerPriorityConfig
  - >> NVIC_SetVectorTable
  - >> NVIC_PriorityGroupConfig
  [Called By]
  - >> main

  NVIC_PriorityGroupConfig (Thumb, 10 bytes, Stack size 0 bytes, stm32f10x_nvic.o(i.NVIC_PriorityGroupConfig))
  [Called By]

  - >> NVIC_Configuration

  NVIC_SetVectorTable (Thumb, 12 bytes, Stack size 0 bytes, stm32f10x_nvic.o(i.NVIC_SetVectorTable))
  [Called By]

  - >> NVIC_Configuration

  NVIC_SystemHandlerPriorityConfig (Thumb, 72 bytes, Stack size 12 bytes, stm32f10x_nvic.o(i.NVIC_SystemHandlerPriorityConfig))
  [Stack]

  - Max Depth = 12
  - Call Chain = NVIC_SystemHandlerPriorityConfig
  [Called By]
  - >> NVIC_Configuration

  PVD_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.PVD_IRQHandler))
  [Address Reference Count : 1]

  - stm32f10x_vector.o(RESET)

  PendSVC (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.PendSVC))
  [Address Reference Count : 1]

  - stm32f10x_vector.o(RESET)

  RCC_APB1PeriphClockCmd (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_rcc.o(i.RCC_APB1PeriphClockCmd))
  [Called By]

  - >> RCC_Configuration

  RCC_APB2PeriphClockCmd (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_rcc.o(i.RCC_APB2PeriphClockCmd))
  [Called By]

  - >> GPIO_Configuration
  - >> RCC_Configuration

  RCC_Configuration (Thumb, 164 bytes, Stack size 8 bytes, gpio.o(i.RCC_Configuration))
  [Stack]

  - Max Depth = 20
  - Call Chain = RCC_Configuration ⇒ RCC_WaitForHSEStartUp
  [Calls]
  - >> RCC_WaitForHSEStartUp
  - >> RCC_SYSCLKConfig
  - >> RCC_PLLConfig
  - >> RCC_PLLCmd
  - >> RCC_PCLK2Config
  - >> RCC_PCLK1Config
  - >> RCC_HSEConfig
  - >> RCC_HCLKConfig
  - >> RCC_GetSYSCLKSource
  - >> RCC_GetFlagStatus
  - >> RCC_DeInit
  - >> RCC_APB2PeriphClockCmd
  - >> RCC_APB1PeriphClockCmd
  - >> FLASH_SetLatency
  - >> FLASH_PrefetchBufferCmd
  [Called By]
  - >> main

  RCC_DeInit (Thumb, 48 bytes, Stack size 0 bytes, stm32f10x_rcc.o(i.RCC_DeInit))
  [Called By]

  - >> RCC_Configuration

  RCC_GetFlagStatus (Thumb, 42 bytes, Stack size 0 bytes, stm32f10x_rcc.o(i.RCC_GetFlagStatus))
  [Called By]

  - >> RCC_WaitForHSEStartUp
  - >> RCC_Configuration

  RCC_GetSYSCLKSource (Thumb, 10 bytes, Stack size 0 bytes, stm32f10x_rcc.o(i.RCC_GetSYSCLKSource))
  [Called By]

  - >> RCC_Configuration

  RCC_HCLKConfig (Thumb, 14 bytes, Stack size 0 bytes, stm32f10x_rcc.o(i.RCC_HCLKConfig))
  [Called By]

  - >> RCC_Configuration

  RCC_HSEConfig (Thumb, 48 bytes, Stack size 0 bytes, stm32f10x_rcc.o(i.RCC_HSEConfig))
  [Called By]

  - >> RCC_Configuration

  RCC_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.RCC_IRQHandler))
  [Address Reference Count : 1]

  - stm32f10x_vector.o(RESET)

  RCC_PCLK1Config (Thumb, 14 bytes, Stack size 0 bytes, stm32f10x_rcc.o(i.RCC_PCLK1Config))
  [Called By]

  - >> RCC_Configuration

  RCC_PCLK2Config (Thumb, 16 bytes, Stack size 0 bytes, stm32f10x_rcc.o(i.RCC_PCLK2Config))
  [Called By]

  - >> RCC_Configuration

  RCC_PLLCmd (Thumb, 6 bytes, Stack size 0 bytes, stm32f10x_rcc.o(i.RCC_PLLCmd))
  [Called By]

  - >> RCC_Configuration

  RCC_PLLConfig (Thumb, 16 bytes, Stack size 0 bytes, stm32f10x_rcc.o(i.RCC_PLLConfig))
  [Called By]

  - >> RCC_Configuration

  RCC_SYSCLKConfig (Thumb, 14 bytes, Stack size 0 bytes, stm32f10x_rcc.o(i.RCC_SYSCLKConfig))
  [Called By]

  - >> RCC_Configuration

  RCC_WaitForHSEStartUp (Thumb, 42 bytes, Stack size 12 bytes, stm32f10x_rcc.o(i.RCC_WaitForHSEStartUp))
  [Stack]

  - Max Depth = 12
  - Call Chain = RCC_WaitForHSEStartUp
  [Calls]
  - >> RCC_GetFlagStatus
  [Called By]
  - >> RCC_Configuration

  RTCAlarm_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.RTCAlarm_IRQHandler))
  [Address Reference Count : 1]

  - stm32f10x_vector.o(RESET)

  RTC_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.RTC_IRQHandler))
  [Address Reference Count : 1]

  - stm32f10x_vector.o(RESET)

  SDIO_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.SDIO_IRQHandler))
  [Address Reference Count : 1]

  - stm32f10x_vector.o(RESET)

  SPI1_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.SPI1_IRQHandler))
  [Address Reference Count : 1]

  - stm32f10x_vector.o(RESET)

  SPI2_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.SPI2_IRQHandler))
  [Address Reference Count : 1]

  - stm32f10x_vector.o(RESET)

  SPI3_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.SPI3_IRQHandler))
  [Address Reference Count : 1]

  - stm32f10x_vector.o(RESET)

  SVCHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.SVCHandler))
  [Address Reference Count : 1]

  - stm32f10x_vector.o(RESET)

  SYSTEMTICK_Isr (Thumb, 34 bytes, Stack size 0 bytes, gpio.o(i.SYSTEMTICK_Isr))
  [Called By]

  - >> SysTickHandler

  SYSTICK_Init (Thumb, 26 bytes, Stack size 8 bytes, gpio.o(i.SYSTICK_Init))
  [Stack]

  - Max Depth = 8
  - Call Chain = SYSTICK_Init
  [Calls]
  - >> SysTick_SetReload
  - >> SysTick_ITConfig
  - >> SysTick_CounterCmd
  [Called By]
  - >> main

  SysTickHandler (Thumb, 4 bytes, Stack size 0 bytes, stm32f10x_it.o(i.SysTickHandler))
  [Calls]

  - >> SYSTEMTICK_Isr
  [Address Reference Count : 1]
  - stm32f10x_vector.o(RESET)

  SysTick_CounterCmd (Thumb, 36 bytes, Stack size 0 bytes, stm32f10x_systick.o(i.SysTick_CounterCmd))
  [Called By]

  - >> SYSTICK_Init

  SysTick_ITConfig (Thumb, 24 bytes, Stack size 0 bytes, stm32f10x_systick.o(i.SysTick_ITConfig))
  [Called By]

  - >> SYSTICK_Init

  SysTick_SetReload (Thumb, 8 bytes, Stack size 0 bytes, stm32f10x_systick.o(i.SysTick_SetReload))
  [Called By]

  - >> SYSTICK_Init

  TAMPER_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.TAMPER_IRQHandler))
  [Address Reference Count : 1]

  - stm32f10x_vector.o(RESET)

  TIM1_BRK_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.TIM1_BRK_IRQHandler))
  [Address Reference Count : 1]

  - stm32f10x_vector.o(RESET)

  TIM1_CC_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.TIM1_CC_IRQHandler))
  [Address Reference Count : 1]

  - stm32f10x_vector.o(RESET)

  TIM1_TRG_COM_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.TIM1_TRG_COM_IRQHandler))
  [Address Reference Count : 1]

  - stm32f10x_vector.o(RESET)

  TIM1_UP_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.TIM1_UP_IRQHandler))
  [Address Reference Count : 1]

  - stm32f10x_vector.o(RESET)

  TIM2_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.TIM2_IRQHandler))
  [Address Reference Count : 1]

  - stm32f10x_vector.o(RESET)

  TIM3_IRQHandler (Thumb, 8 bytes, Stack size 0 bytes, stm32f10x_it.o(i.TIM3_IRQHandler))
  [Calls]

  - >> TIM_ClearITPendingBit
  [Address Reference Count : 1]
  - stm32f10x_vector.o(RESET)

  TIM4_IRQHandler (Thumb, 8 bytes, Stack size 0 bytes, stm32f10x_it.o(i.TIM4_IRQHandler))
  [Calls]

  - >> TIM_ClearITPendingBit
  [Address Reference Count : 1]
  - stm32f10x_vector.o(RESET)

  TIM5_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.TIM5_IRQHandler))
  [Address Reference Count : 1]

  - stm32f10x_vector.o(RESET)

  TIM6_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.TIM6_IRQHandler))
  [Address Reference Count : 1]

  - stm32f10x_vector.o(RESET)

  TIM7_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.TIM7_IRQHandler))
  [Address Reference Count : 1]

  - stm32f10x_vector.o(RESET)

  TIM8_BRK_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.TIM8_BRK_IRQHandler))
  [Address Reference Count : 1]

  - stm32f10x_vector.o(RESET)

  TIM8_CC_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.TIM8_CC_IRQHandler))
  [Address Reference Count : 1]

  - stm32f10x_vector.o(RESET)

  TIM8_TRG_COM_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.TIM8_TRG_COM_IRQHandler))
  [Address Reference Count : 1]

  - stm32f10x_vector.o(RESET)

  TIM8_UP_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.TIM8_UP_IRQHandler))
  [Address Reference Count : 1]

  - stm32f10x_vector.o(RESET)

  TIM_ClearITPendingBit (Thumb, 6 bytes, Stack size 0 bytes, stm32f10x_tim.o(i.TIM_ClearITPendingBit))
  [Called By]

  - >> TIM4_IRQHandler
  - >> TIM3_IRQHandler

  UART4_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.UART4_IRQHandler))
  [Address Reference Count : 1]

  - stm32f10x_vector.o(RESET)

  UART5_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.UART5_IRQHandler))
  [Address Reference Count : 1]

  - stm32f10x_vector.o(RESET)

  USART1_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.USART1_IRQHandler))
  [Address Reference Count : 1]

  - stm32f10x_vector.o(RESET)

  USART2_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.USART2_IRQHandler))
  [Address Reference Count : 1]

  - stm32f10x_vector.o(RESET)

  USART3_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.USART3_IRQHandler))
  [Address Reference Count : 1]

  - stm32f10x_vector.o(RESET)

  USBWakeUp_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.USBWakeUp_IRQHandler))
  [Address Reference Count : 1]

  - stm32f10x_vector.o(RESET)

  USB_HP_CAN_TX_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.USB_HP_CAN_TX_IRQHandler))
  [Address Reference Count : 1]

  - stm32f10x_vector.o(RESET)

  USB_LP_CAN_RX0_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.USB_LP_CAN_RX0_IRQHandler))
  [Address Reference Count : 1]

  - stm32f10x_vector.o(RESET)

  UsageFaultException (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.UsageFaultException))
  [Calls]

  - >> UsageFaultException
  [Called By]
  - >> UsageFaultException
  [Address Reference Count : 1]
  - stm32f10x_vector.o(RESET)

  WWDG_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.WWDG_IRQHandler))
  [Address Reference Count : 1]

  - stm32f10x_vector.o(RESET)

  __scatterload_copy (Thumb, 14 bytes, Stack size unknown bytes, handlers.o(i.__scatterload_copy), UNUSED)

  __scatterload_null (Thumb, 2 bytes, Stack size unknown bytes, handlers.o(i.__scatterload_null), UNUSED)

  __scatterload_zeroinit (Thumb, 14 bytes, Stack size unknown bytes, handlers.o(i.__scatterload_zeroinit), UNUSED)

  main (Thumb, 104 bytes, Stack size 8 bytes, main.o(i.main))
  [Stack]

  - Max Depth = 112
  - Call Chain = main ⇒ LCD_Print ⇒ LCD_P16x16Str ⇒ LCD_Set_Pos ⇒ LCD_WrCmd
  [Calls]
  - >> SYSTICK_Init
  - >> RCC_Configuration
  - >> NVIC_Configuration
  - >> LCD_Print
  - >> LCD_Init
  - >> GPIO_UserInit
  - >> EXTI_Configuration
  - >> Draw_BMP
  [Address Reference Count : 1]
  - entry9a.o(.ARM.Collect$$$$0000000B)

  ### Local Symbols

  ### Undefined Global Symbols